Task: Form a communication between Two R-pi

Hw: R-Pi both are connected over physical ethernet layer

Sw: Both R-pi Has Linux Operating System

Socket IPC mechanisam will be used

Message is not continues Streaming, Packet type Message

Payload should be in Json Format.